DIVISION

TEMPLATES AND GUIDESFG

EXAMPLE CONFIGURATION FOR BASIC NAMED EIGRP:

router eigrp SEAHAWK

!

address-family ipv4 unicast autonomous-system 3

eigrp router-id 1.1.1.1

network 10.0.0.0 0.0.0.255

network 192.168.15.1 0.0.0.0

!

af-interface default

passive-interface

!

af-interface tunnel 100

no passive-interface

authentication mode md5

authentication key-chain SUPERBOWL

summary-address 172.16.0.0 255.255.0.0 leak-map ABC

!

topology base

redistribute ospf 20 route-map XYZ

default-metric 10000 0 255 1 1500

variance 2

distribute-list 100 in tunnel 1

no auto-summary