DIVISION

TEMPLATES AND GUIDESFG

All applicable network devices within the network shall have archive capabilities configured as follows:

!

configure terminal

!

archive

log config

logging enable

logging size 250

hidekeys

path tftp://22.17.17.30/student\_rtr\_**# (where # is your student number)**

write-memory

time-period 2880

!

end

!

wr

!