DIVISION

TEMPLATES AND GUIDESFG

How to configure Net Flow

flow exporter XXXX

destination X.X.X.X

source XXXX *(INTERFACE)*

ttl 7

transport udp 9996

!

flow monitor XXXX

exporter XXXX

cache timeout inactive 20

cache timeout active 180

record netflow-original

!

Int XXXXX

Ip flow monitor XXXX input

Ip flow monitor XXXX output