DIVISION

TEMPLATES AND GUIDESFG

ADDING, REMOVING AND OVERWRITING VLANs ALLOWED ON A TRUNK

1. TO OVERWRITE THE VLANs ALLOWED ON A TRUNK:

INT G0/0

SWITCHPORT MODE TRUNK

SWITCHPORT TRUNK ALLOW VLAN 2-7

\*NOTE, THIS COMPLETELY OVERWRITES WHATEVER VLANS WERE ALLOWED ON THE TRUNK BEFORE AND THE TRUNK NOW *ONLY* ALLOWS VLANS 2-7.

1. TO ADD VLANs ALLOWED ON A TRUNK:

INT G0/0

SWITCHPORT MODE TRUNK

SWITCHPORT TRUNK ALLOW VLAN ADD 9

\*NOTE, THIS ADDS VLAN 9 TO THE LIST OF VLANS THAT WERE PREVIOUSLY ALLOWED ON THE TRUNK. IF THE TRUNK PREVIOUSLY ALLOWED VLANS 2-7, IT NOW ALLOWS 2-7, AND 9.

1. TO REMOVE VLANs ALLOWED ON A TRUNK:

INT G0/0

SWITCHPORT MODE TRUNK

SWITCHPORT TRUNK ALLOW VLAN REMOVE 5

\*NOTE, THIS REMOVES ONLY VLAN 5 FROM THE LIST OF VLANS ALLOWED ON THE TRUNK