DIVISION

TEMPLATES AND GUIDESFG

BASIC VRF CONFIGURATION:

Vrf definition ABC

Address-family ipv4

Address-family ipv6

Interface G0/0/0.10

Encap dot1q 10

Vrf forwarding ABC

Ip address 10.10.10.10 255.255.255.0

\*\*NOTE: If you apply the command “Vrf forwarding ABC” (which assigns the interface to that vrf) any IP address that was on the interface will be removed because it was associated with its assignment to the global routing table. The IP address will need to be re-applied after the command “vrf forwarding ABC” has been configured.