DIVISION

TEMPLATES AND GUIDESFG

EXAMPLE OF USING TFTP TO EXTRACT A FILE:

SWITCH#

Config t

Ip tftp source vlan 1xx 🡨 specify the TFTP source for your switch to be an interface that can reach the TFTP destination

Exit 🡨 back out of configuration mode

Copy tftp flash

Address or name of remote host [ ]? x.x.x.x 🡨 ip address you want to extract a file from

Source filename [ ]? xxxxx.xxxx 🡨 name of the file you want to extract

Destination filename [ ]? xxxxx.xxxx 🡨 name you want to save the file as

You should see a message that looks similar to this:

Accessing tftp://x.x.x.x/xxxxxxx...

Loading xxxxxx from x.x.x.x (via Vlanxxx): !!!

[OK - 16 bytes]

16 bytes copied in 8.020 secs (2 bytes/sec)