DIVISION

TEMPLATES AND GUIDESFG

HOW TO USE CONFIGURE ALIAS COMMANDS:

ALIAS Command Examples:

The following alias command could be applied if the administrator wanted to use the command “abc” as a shortcut for viewing the OSPFv3 IPV6 neighbor status for a vrf called RED:

**Alias exec abc show ospfv3 ipv6 vrf RED neighbor**

The following alias command could be applied if the administrator wanted to use the command “x4” as a shortcut for viewing the running configuration of interface g1/0/4:

**Alias exec x4 show run interface g1/0/4**

The following alias command could be applied if the administrator wanted to use the command “b256” as a shortcut for configuring a bgp router process number 65256:

**Alias configure b256 router bgp 65256**